Checklist LaneLED INOX42

[ ]  Quotation [ ]  Order

|  |
| --- |
| **Contact Details** |
| Customer:  | Consultant:  | Project:  |
| Customer-No.:  | Contact person:  | Delivery date:  |
|  |  |  |

|  |
| --- |
| **Calculation for: [ ]** Pathway [ ]  Stairway [ ]   |
| **Project description:**  |

|  |
| --- |
| **Consultant involved:** [ ]  yes [ ]  no |
| **Existing quotation?** [ ]  yes [ ]  no |
| **Desired LaneLED type:** [ ]  cold white approx. 5'500 K [ ]  comfort white approx. 4'000 – 4'400 K |
| **Feed-in cable lenght:** *..........*m (mention exact feed-in point in sketch) |
| **Placement:** [ ]  indoor [ ]  outdoor [ ]  private installation [ ]  public installation |
| **Surface type** [ ]  concrete [ ]  asphalt [ ]  wood**(installation ground):** [ ]  …………………… [ ]  isolation (outdoor wall) |
| **Ligting requirement:** *...........*lxMin. luminance intensity according to DIN EN12464-1: * Pedestrian undercrossing with low number of persons: **50lx**
* Pedestrian undercrossing with high number of persons, stairways, corridors, traffic zones: **100lx** but depending on the exact utilisation of the corresponding room
 |

|  |
| --- |
| **CAD-Files available:**[ ]  DXF-file[ ]  DWG-file |

|  |
| --- |
| **Comments:**  |

|  |
| --- |
| **Attachement:** [ ]  Pictures [ ]  Sketches  |

|  |
| --- |
| **Stairway (hand rail on the wall):** |
| **Stairway (hand rail on poles):** |
| **Pathway (hand rail on poles):** |
| **Pathway (hand rail on top of balustrade):** |
| **Pathway (hand rail on wall):** |