Checklist LaneLED INOX42

Quotation  Order

|  |
| --- |
| **Contact Details** |
| Customer: | Consultant: | Project: |
| Customer-No.: | Contact person: | Delivery date: |
|  |  |  |

|  |
| --- |
| **Calculation for:** Pathway  Stairway |
| **Project description:** |

|  |
| --- |
| **Consultant involved:**  yes  no |
| **Existing quotation?**  yes  no |
| **Desired LaneLED type:**  cold white approx. 5'500 K  comfort white approx. 4'000 – 4'400 K |
| **Feed-in cable lenght:** *..........*m (mention exact feed-in point in sketch) |
| **Placement:**  indoor  outdoor  private installation  public installation |
| **Surface type**  concrete  asphalt  wood  **(installation ground):**  ……………………  isolation (outdoor wall) |
| **Ligting requirement:** *...........*lx  Min. luminance intensity according to DIN EN12464-1:   * Pedestrian undercrossing with low number of persons: **50lx** * Pedestrian undercrossing with high number of persons, stairways, corridors, traffic zones: **100lx** but depending on the exact utilisation of the corresponding room |

|  |
| --- |
| **CAD-Files available:**  DXF-file  DWG-file |

|  |
| --- |
| **Comments:** |

|  |
| --- |
| **Attachement:**  Pictures  Sketches |

|  |
| --- |
| **Stairway (hand rail on the wall):** |
| **Stairway (hand rail on poles):** |
| **Pathway (hand rail on poles):** |
| **Pathway (hand rail on top of balustrade):** |
| **Pathway (hand rail on wall):** |